# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Constants | Fields | Methods | Inherited Methods

# CamcorderProfile

`public class CamcorderProfile`
`extends Object` ``

java.lang.Object
↳ | android.media.CamcorderProfile

Retrieves the predefined camcorder profile settings for camcorder applications. These settings are read-only.

The compressed output from a recording session with a given CamcorderProfile contains two tracks: one for audio and one for video.

Each profile specifies the following set of parameters:

- The file output format
- Video codec format
- Video bit rate in bits per second
- Video frame rate in frames per second
- Video frame width and height,
- Audio codec format
- Audio bit rate in bits per second,
- Audio sample rate
- Number of audio channels for recording.

## Summary

### Constants
`int` | `QUALITY_1080P` Quality level corresponding to the 1080p (1920 x 1080) resolution.
`int` | `QUALITY_2160P` Quality level corresponding to the 2160p (3840x2160) resolution.
`int` | `QUALITY_2K` Quality level corresponding to 2K (2048 x 1080) resolution
`int` | `QUALITY_480P` Quality level corresponding to the 480p (720 x 480) resolution.
`int` | `QUALITY_4KDCI` Quality level corresponding to 4k-DCI (4096 x 2160) resolution.
`int` | `QUALITY_720P` Quality level corresponding to the 720p (1280 x 720) resolution.
`int` | `QUALITY_8KUHD` Quality level corresponding to 8K UHD (7680 x 4320) resolution
`int` | `QUALITY_CIF` Quality level corresponding to the cif (352 x 288) resolution.
`int` | `QUALITY_HIGH` Quality level corresponding to the highest available resolution.
`int` | `QUALITY_HIGH_SPEED_1080P` High speed ( >= 100fps) quality level corresponding to the 1080p (1920 x 1080 or 1920x1088) resolution.
`int` | `QUALITY_HIGH_SPEED_2160P` High speed ( >= 100fps) quality level corresponding to the 2160p (3840 x 2160) resolution.
`int` | `QUALITY_HIGH_SPEED_480P` High speed ( >= 100fps) quality level corresponding to the 480p (720 x 480) resolution.
`int` | `QUALITY_HIGH_SPEED_4KDCI` High speed ( >= 100fps) quality level corresponding to the 4K-DCI (4096 x 2160)
`int` | `QUALITY_HIGH_SPEED_720P` High speed ( >= 100fps) quality level corresponding to the 720p (1280 x 720) resolution.
`int` | `QUALITY_HIGH_SPEED_CIF` High speed ( >= 100fps) quality level corresponding to the CIF (352 x 288)
`int` | `QUALITY_HIGH_SPEED_HIGH` High speed ( >= 100fps) quality level corresponding to the highest available resolution.
`int` | `QUALITY_HIGH_SPEED_LOW` High speed ( >= 100fps) quality level corresponding to the lowest available resolution.
`int` | `QUALITY_HIGH_SPEED_VGA` High speed ( >= 100fps) quality level corresponding to the VGA (640 x 480)
`int` | `QUALITY_LOW` Quality level corresponding to the lowest available resolution.
`int` | `QUALITY_QCIF` Quality level corresponding to the qcif (176 x 144) resolution.
`int` | `QUALITY_QHD` Quality level corresponding to QHD (2560 x 1440) resolution
`int` | `QUALITY_QVGA` Quality level corresponding to the QVGA (320x240) resolution.
`int` | `QUALITY_TIME_LAPSE_1080P` Time lapse quality level corresponding to the 1080p (1920 x 1088) resolution.
`int` | `QUALITY_TIME_LAPSE_2160P` Time lapse quality level corresponding to the 2160p (3840 x 2160) resolution.
`int` | `QUALITY_TIME_LAPSE_2K` Time lapse quality level corresponding to the 2K (2048 x 1080) resolution.
`int` | `QUALITY_TIME_LAPSE_480P` Time lapse quality level corresponding to the 480p (720 x 480) resolution.
`int` | `QUALITY_TIME_LAPSE_4KDCI` Time lapse quality level corresponding to the 4k-DCI (4096 x 2160) resolution.
`int` | `QUALITY_TIME_LAPSE_720P` Time lapse quality level corresponding to the 720p (1280 x 720) resolution.
`int` | `QUALITY_TIME_LAPSE_8KUHD` Time lapse quality level corresponding to the 8K UHD (7680 x 4320) resolution.
`int` | `QUALITY_TIME_LAPSE_CIF` Time lapse quality level corresponding to the cif (352 x 288) resolution.
`int` | `QUALITY_TIME_LAPSE_HIGH` Time lapse quality level corresponding to the highest available resolution.
`int` | `QUALITY_TIME_LAPSE_LOW` Time lapse quality level corresponding to the lowest available resolution.
`int` | `QUALITY_TIME_LAPSE_QCIF` Time lapse quality level corresponding to the qcif (176 x 144) resolution.
`int` | `QUALITY_TIME_LAPSE_QHD` Time lapse quality level corresponding to the QHD (2560 x 1440) resolution.
`int` | `QUALITY_TIME_LAPSE_QVGA` Time lapse quality level corresponding to the QVGA (320 x 240) resolution.
`int` | `QUALITY_TIME_LAPSE_VGA` Time lapse quality level corresponding to the VGA (640 x 480) resolution.
`int` | `QUALITY_VGA` Quality level corresponding to the VGA (640 x 480) resolution.

### Fields
`public int` | `audioBitRate` The target audio output bit rate in bits per second
`public int` | `audioChannels` The number of audio channels used for the audio track
`public int` | `audioCodec` The audio encoder being used for the audio track.
`public int` | `audioSampleRate` The audio sampling rate used for the audio track
`public int` | `duration` Default recording duration in seconds before the session is terminated.
`public int` | `fileFormat` The file output format of the camcorder profile
`public int` | `quality` The quality level of the camcorder profile
`public int` | `videoBitRate` The target video output bit rate in bits per second This is the target recorded video output bit rate if the application configures the video recording via `MediaRecorder#setProfile` without specifying any other `MediaRecorder` encoding parameters.
`public int` | `videoCodec` The video encoder being used for the video track
`public int` | `videoFrameHeight` The target video frame height in pixels
`public int` | `videoFrameRate` The target video frame rate in frames per second.
`public int` | `videoFrameWidth` The target video frame width in pixels

### Public methods
`static CamcorderProfile` | `get(int quality)` This method is deprecated. Use `getAll(String, int)` instead
`static CamcorderProfile` | `get(int cameraId, int quality)` This method is deprecated. Use `getAll(String, int)` instead
`static EncoderProfiles` | `getAll(String cameraId, int quality)` Returns all encoder profiles of a camcorder profile for the given camera at the given quality level.
`static boolean` | `hasProfile(int cameraId, int quality)` Returns true if a camcorder profile exists for the given camera at the given quality level.
`static boolean` | `hasProfile(int quality)` Returns true if a camcorder profile exists for the first back-facing camera at the given quality level.

### Inherited methods
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.

## Constants

### QUALITY_1080P

    public static final int QUALITY_1080P

Quality level corresponding to the 1080p (1920 x 1080) resolution. Note that the vertical resolution for 1080p can also be 1088, instead of 1080 (used by some vendors to avoid cropping during video playback).

Constant Value: 6 (0x00000006)

### QUALITY_2160P

    public static final int QUALITY_2160P

Quality level corresponding to the 2160p (3840x2160) resolution.

Constant Value: 8 (0x00000008)

### QUALITY_2K

    public static final int QUALITY_2K

Quality level corresponding to 2K (2048 x 1080) resolution

Constant Value: 12 (0x0000000c)

### QUALITY_480P

    public static final int QUALITY_480P

Quality level corresponding to the 480p (720 x 480) resolution. Note that the horizontal resolution for 480p can also be other values, such as 640 or 704, instead of 720.

Constant Value: 4 (0x00000004)

### QUALITY_4KDCI

    public static final int QUALITY_4KDCI

Quality level corresponding to 4k-DCI (4096 x 2160) resolution.

Constant Value: 10 (0x0000000a)

### QUALITY_720P

    public static final int QUALITY_720P

Quality level corresponding to the 720p (1280 x 720) resolution.

Constant Value: 5 (0x00000005)

### QUALITY_8KUHD

    public static final int QUALITY_8KUHD

Quality level corresponding to 8K UHD (7680 x 4320) resolution

Constant Value: 13 (0x0000000d)

### QUALITY_CIF

    public static final int QUALITY_CIF

Quality level corresponding to the cif (352 x 288) resolution.

Constant Value: 3 (0x00000003)

### QUALITY_HIGH

    public static final int QUALITY_HIGH

Quality level corresponding to the highest available resolution.

Constant Value: 1 (0x00000001)

### QUALITY_HIGH_SPEED_1080P

    public static final int QUALITY_HIGH_SPEED_1080P

High speed ( >= 100fps) quality level corresponding to the 1080p (1920 x 1080 or 1920x1088) resolution.

Constant Value: 2004 (0x000007d4)

### QUALITY_HIGH_SPEED_2160P

    public static final int QUALITY_HIGH_SPEED_2160P

High speed ( >= 100fps) quality level corresponding to the 2160p (3840 x 2160) resolution.

Constant Value: 2005 (0x000007d5)

### QUALITY_HIGH_SPEED_480P

    public static final int QUALITY_HIGH_SPEED_480P

High speed ( >= 100fps) quality level corresponding to the 480p (720 x 480) resolution. Note that the horizontal resolution for 480p can also be other values, such as 640 or 704, instead of 720.

Constant Value: 2002 (0x000007d2)

### QUALITY_HIGH_SPEED_4KDCI

    public static final int QUALITY_HIGH_SPEED_4KDCI

High speed ( >= 100fps) quality level corresponding to the 4K-DCI (4096 x 2160)

Constant Value: 2008 (0x000007d8)

### QUALITY_HIGH_SPEED_720P

    public static final int QUALITY_HIGH_SPEED_720P

High speed ( >= 100fps) quality level corresponding to the 720p (1280 x 720) resolution.

Constant Value: 2003 (0x000007d3)

### QUALITY_HIGH_SPEED_CIF

    public static final int QUALITY_HIGH_SPEED_CIF

High speed ( >= 100fps) quality level corresponding to the CIF (352 x 288)

Constant Value: 2006 (0x000007d6)

### QUALITY_HIGH_SPEED_HIGH

    public static final int QUALITY_HIGH_SPEED_HIGH

High speed ( >= 100fps) quality level corresponding to the highest available resolution.

Constant Value: 2001 (0x000007d1)

### QUALITY_HIGH_SPEED_LOW

    public static final int QUALITY_HIGH_SPEED_LOW

High speed ( >= 100fps) quality level corresponding to the lowest available resolution.

For all the high speed profiles defined below ((from `QUALITY_HIGH_SPEED_LOW` to `QUALITY_HIGH_SPEED_2160P`), they are similar as normal recording profiles, with just higher output frame rate and bit rate. Therefore, setting these profiles with `MediaRecorder#setProfile` without specifying any other encoding parameters will produce high speed videos rather than slow motion videos that have different capture and output (playback) frame rates. To record slow motion videos, the application must set video output (playback) frame rate and bit rate appropriately via `MediaRecorder#setVideoFrameRate` and `MediaRecorder#setVideoEncodingBitRate` based on the slow motion factor. If the application intends to do the video recording with `MediaCodec` encoder, it must set each individual field of `MediaFormat` similarly according to this CamcorderProfile.

See also:

- `videoBitRate`
- `videoFrameRate`
- `MediaRecorder`
- `MediaCodec`
- `MediaFormat`

Constant Value: 2000 (0x000007d0)

### QUALITY_HIGH_SPEED_VGA

    public static final int QUALITY_HIGH_SPEED_VGA

High speed ( >= 100fps) quality level corresponding to the VGA (640 x 480)

Constant Value: 2007 (0x000007d7)

### QUALITY_LOW

    public static final int QUALITY_LOW

Quality level corresponding to the lowest available resolution.

Constant Value: 0 (0x00000000)

### QUALITY_QCIF

    public static final int QUALITY_QCIF

Quality level corresponding to the qcif (176 x 144) resolution.

Constant Value: 2 (0x00000002)

### QUALITY_QHD

    public static final int QUALITY_QHD

Quality level corresponding to QHD (2560 x 1440) resolution

Constant Value: 11 (0x0000000b)

### QUALITY_QVGA

    public static final int QUALITY_QVGA

Quality level corresponding to the QVGA (320x240) resolution.

Constant Value: 7 (0x00000007)

### QUALITY_TIME_LAPSE_1080P

    public static final int QUALITY_TIME_LAPSE_1080P

Time lapse quality level corresponding to the 1080p (1920 x 1088) resolution.

Constant Value: 1006 (0x000003ee)

### QUALITY_TIME_LAPSE_2160P

    public static final int QUALITY_TIME_LAPSE_2160P

Time lapse quality level corresponding to the 2160p (3840 x 2160) resolution.

Constant Value: 1008 (0x000003f0)

### QUALITY_TIME_LAPSE_2K

    public static final int QUALITY_TIME_LAPSE_2K

Time lapse quality level corresponding to the 2K (2048 x 1080) resolution.

Constant Value: 1012 (0x000003f4)

### QUALITY_TIME_LAPSE_480P

    public static final int QUALITY_TIME_LAPSE_480P

Time lapse quality level corresponding to the 480p (720 x 480) resolution.

Constant Value: 1004 (0x000003ec)

### QUALITY_TIME_LAPSE_4KDCI

    public static final int QUALITY_TIME_LAPSE_4KDCI

Time lapse quality level corresponding to the 4k-DCI (4096 x 2160) resolution.

Constant Value: 1010 (0x000003f2)

### QUALITY_TIME_LAPSE_720P

    public static final int QUALITY_TIME_LAPSE_720P

Time lapse quality level corresponding to the 720p (1280 x 720) resolution.

Constant Value: 1005 (0x000003ed)

### QUALITY_TIME_LAPSE_8KUHD

    public static final int QUALITY_TIME_LAPSE_8KUHD

Time lapse quality level corresponding to the 8K UHD (7680 x 4320) resolution.

Constant Value: 1013 (0x000003f5)

### QUALITY_TIME_LAPSE_CIF

    public static final int QUALITY_TIME_LAPSE_CIF

Time lapse quality level corresponding to the cif (352 x 288) resolution.

Constant Value: 1003 (0x000003eb)

### QUALITY_TIME_LAPSE_HIGH

    public static final int QUALITY_TIME_LAPSE_HIGH

Time lapse quality level corresponding to the highest available resolution.

Constant Value: 1001 (0x000003e9)

### QUALITY_TIME_LAPSE_LOW

    public static final int QUALITY_TIME_LAPSE_LOW

Time lapse quality level corresponding to the lowest available resolution.

Constant Value: 1000 (0x000003e8)

### QUALITY_TIME_LAPSE_QCIF

    public static final int QUALITY_TIME_LAPSE_QCIF

Time lapse quality level corresponding to the qcif (176 x 144) resolution.

Constant Value: 1002 (0x000003ea)

### QUALITY_TIME_LAPSE_QHD

    public static final int QUALITY_TIME_LAPSE_QHD

Time lapse quality level corresponding to the QHD (2560 x 1440) resolution.

Constant Value: 1011 (0x000003f3)

### QUALITY_TIME_LAPSE_QVGA

    public static final int QUALITY_TIME_LAPSE_QVGA

Time lapse quality level corresponding to the QVGA (320 x 240) resolution.

Constant Value: 1007 (0x000003ef)

### QUALITY_TIME_LAPSE_VGA

    public static final int QUALITY_TIME_LAPSE_VGA

Time lapse quality level corresponding to the VGA (640 x 480) resolution.

Constant Value: 1009 (0x000003f1)

### QUALITY_VGA

    public static final int QUALITY_VGA

Quality level corresponding to the VGA (640 x 480) resolution.

Constant Value: 9 (0x00000009)

## Fields

### audioBitRate

    public int audioBitRate

The target audio output bit rate in bits per second

### audioChannels

    public int audioChannels

The number of audio channels used for the audio track

### audioCodec

    public int audioCodec

The audio encoder being used for the audio track.

See also:

- `MediaRecorder.AudioEncoder`

### audioSampleRate

    public int audioSampleRate

The audio sampling rate used for the audio track

### duration

    public int duration

Default recording duration in seconds before the session is terminated. This is useful for applications like MMS has limited file size requirement.

### fileFormat

    public int fileFormat

The file output format of the camcorder profile

See also:

- `MediaRecorder.OutputFormat`

### quality

    public int quality

The quality level of the camcorder profile

### videoBitRate

    public int videoBitRate

The target video output bit rate in bits per second

This is the target recorded video output bit rate if the application configures the video recording via `MediaRecorder#setProfile` without specifying any other `MediaRecorder` encoding parameters. For example, for high speed quality profiles (from `QUALITY_HIGH_SPEED_LOW` to `QUALITY_HIGH_SPEED_2160P`), this is the bit rate where the video is recorded with. If the application intends to record slow motion videos with the high speed quality profiles, it must set a different video bit rate that is corresponding to the desired recording output bit rate (i.e., the encoded video bit rate during normal playback) via `MediaRecorder#setVideoEncodingBitRate`. For example, if `QUALITY_HIGH_SPEED_720P` advertises 240fps `videoFrameRate` and 64Mbps `videoBitRate` in the high speed CamcorderProfile, and the application intends to record 1/8 factor slow motion recording videos, the application must set 30fps via `MediaRecorder#setVideoFrameRate` and 8Mbps ( `videoBitRate` * slow motion factor) via `MediaRecorder#setVideoEncodingBitRate`. Failing to do so will result in videos with unexpected frame rate and bit rate, or `MediaRecorder` error if the output bit rate exceeds the encoder limit. If the application intends to do the video recording with `MediaCodec` encoder, it must set each individual field of `MediaFormat` similarly according to this CamcorderProfile.

See also:

- `videoFrameRate`
- `MediaRecorder`
- `MediaCodec`
- `MediaFormat`

### videoCodec

    public int videoCodec

The video encoder being used for the video track

See also:

- `MediaRecorder.VideoEncoder`

### videoFrameHeight

    public int videoFrameHeight

The target video frame height in pixels

### videoFrameRate

    public int videoFrameRate

The target video frame rate in frames per second.

This is the target recorded video output frame rate per second if the application configures the video recording via `MediaRecorder#setProfile` without specifying any other `MediaRecorder` encoding parameters. For example, for high speed quality profiles (from `QUALITY_HIGH_SPEED_LOW` to `QUALITY_HIGH_SPEED_2160P`), this is the frame rate where the video is recorded and played back with. If the application intends to create slow motion use case with the high speed quality profiles, it must set a different video frame rate that is corresponding to the desired output (playback) frame rate via `MediaRecorder#setVideoFrameRate`. For example, if `QUALITY_HIGH_SPEED_720P` advertises 240fps `videoFrameRate` in the CamcorderProfile, and the application intends to create 1/8 factor slow motion recording videos, the application must set 30fps via `MediaRecorder#setVideoFrameRate`. Failing to do so will result in high speed videos with normal speed playback frame rate (240fps for above example). If the application intends to do the video recording with `MediaCodec` encoder, it must set each individual field of `MediaFormat` similarly according to this CamcorderProfile.

See also:

- `videoBitRate`
- `MediaRecorder`
- `MediaCodec`
- `MediaFormat`

### videoFrameWidth

    public int videoFrameWidth

The target video frame width in pixels

## Public methods

### get

    public static CamcorderProfile get (int quality)

This method is deprecated.
Use `getAll(String, int)` instead

Returns the default camcorder profile at the given quality level for the first back-facing camera on the device. If the device has no back-facing camera, this returns null.

Parameters
`quality` | `int`: the target quality level for the camcorder profile

Returns
`CamcorderProfile` |

See also:

- `get(int, int)`

### get

    public static CamcorderProfile get (int cameraId,
                    int quality)

This method is deprecated.
Use `getAll(String, int)` instead

Returns the default camcorder profile for the given camera at the given quality level. Quality levels QUALITY_LOW, QUALITY_HIGH are guaranteed to be supported, while other levels may or may not be supported. The supported levels can be checked using `hasProfile(int, int)`. QUALITY_LOW refers to the lowest quality available, while QUALITY_HIGH refers to the highest quality available. QUALITY_LOW/QUALITY_HIGH have to match one of qcif, cif, 480p, 720p, 1080p or 2160p. E.g. if the device supports 480p, 720p, 1080p and 2160p, then low is 480p and high is 2160p. The same is true for time lapse quality levels, i.e. QUALITY_TIME_LAPSE_LOW, QUALITY_TIME_LAPSE_HIGH are guaranteed to be supported and have to match one of qcif, cif, 480p, 720p, 1080p, or 2160p. For high speed quality levels, they may or may not be supported. If a subset of the levels are supported, QUALITY_HIGH_SPEED_LOW and QUALITY_HIGH_SPEED_HIGH are guaranteed to be supported and have to match one of 480p, 720p, or 1080p. A camcorder recording session with higher quality level usually has higher output bit rate, better video and/or audio recording quality, larger video frame resolution and higher audio sampling rate, etc, than those with lower quality level.

Parameters
`cameraId` | `int`: the id for the camera. Integer camera ids parsed from the list received by invoking `CameraManager#getCameraIdList` can be used as long as they are `CameraMetadata#REQUEST_AVAILABLE_CAPABILITIES_BACKWARD_COMPATIBLE` and not `EXTERNAL`.
`quality` | `int`: the target quality level for the camcorder profile.

Returns
`CamcorderProfile` |

Throws
`IllegalArgumentException` | if quality is not one of the defined QUALITY_ values.

See also:

- `QUALITY_LOW`
- `QUALITY_HIGH`
- `QUALITY_QCIF`
- `QUALITY_CIF`
- `QUALITY_480P`
- `QUALITY_720P`
- `QUALITY_1080P`
- `QUALITY_2160P`
- `QUALITY_TIME_LAPSE_LOW`
- `QUALITY_TIME_LAPSE_HIGH`
- `QUALITY_TIME_LAPSE_QCIF`
- `QUALITY_TIME_LAPSE_CIF`
- `QUALITY_TIME_LAPSE_480P`
- `QUALITY_TIME_LAPSE_720P`
- `QUALITY_TIME_LAPSE_1080P`
- `QUALITY_TIME_LAPSE_2160P`
- `QUALITY_HIGH_SPEED_LOW`
- `QUALITY_HIGH_SPEED_HIGH`
- `QUALITY_HIGH_SPEED_480P`
- `QUALITY_HIGH_SPEED_720P`
- `QUALITY_HIGH_SPEED_1080P`
- `QUALITY_HIGH_SPEED_2160P`

### getAll

    public static EncoderProfiles getAll (String cameraId,
                    int quality)

Returns all encoder profiles of a camcorder profile for the given camera at the given quality level. Quality levels QUALITY_LOW, QUALITY_HIGH are guaranteed to be supported, while other levels may or may not be supported. The supported levels can be checked using `hasProfile(int, int)`. QUALITY_LOW refers to the lowest quality available, while QUALITY_HIGH refers to the highest quality available. QUALITY_LOW/QUALITY_HIGH have to match one of qcif, cif, 480p, 720p, 1080p or 2160p. E.g. if the device supports 480p, 720p, 1080p and 2160p, then low is 480p and high is 2160p. The same is true for time lapse quality levels, i.e. QUALITY_TIME_LAPSE_LOW, QUALITY_TIME_LAPSE_HIGH are guaranteed to be supported and have to match one of qcif, cif, 480p, 720p, 1080p, or 2160p. For high speed quality levels, they may or may not be supported. If a subset of the levels are supported, QUALITY_HIGH_SPEED_LOW and QUALITY_HIGH_SPEED_HIGH are guaranteed to be supported and have to match one of 480p, 720p, or 1080p. A camcorder recording session with higher quality level usually has higher output bit rate, better video and/or audio recording quality, larger video frame resolution and higher audio sampling rate, etc, than those with lower quality level.

Parameters
`cameraId` | `String`: the id for the camera. Numeric camera ids from the list received by invoking `CameraManager#getCameraIdList` can be used as long as they are `CameraMetadata#REQUEST_AVAILABLE_CAPABILITIES_BACKWARD_COMPATIBLE` and not `EXTERNAL`. This value cannot be `null`.
`quality` | `int`: the target quality level for the camcorder profile. Value is `QUALITY_LOW`, `QUALITY_HIGH`, `QUALITY_QCIF`, `QUALITY_CIF`, `QUALITY_480P`, `QUALITY_720P`, `QUALITY_1080P`, `QUALITY_QVGA`, `QUALITY_2160P`, `QUALITY_VGA`, `QUALITY_4KDCI`, `QUALITY_QHD`, `QUALITY_2K`, `QUALITY_8KUHD`, `QUALITY_TIME_LAPSE_LOW`, `QUALITY_TIME_LAPSE_HIGH`, `QUALITY_TIME_LAPSE_QCIF`, `QUALITY_TIME_LAPSE_CIF`, `QUALITY_TIME_LAPSE_480P`, `QUALITY_TIME_LAPSE_720P`, `QUALITY_TIME_LAPSE_1080P`, `QUALITY_TIME_LAPSE_QVGA`, `QUALITY_TIME_LAPSE_2160P`, `QUALITY_TIME_LAPSE_VGA`, `QUALITY_TIME_LAPSE_4KDCI`, `QUALITY_TIME_LAPSE_QHD`, `QUALITY_TIME_LAPSE_2K`, `QUALITY_TIME_LAPSE_8KUHD`, `QUALITY_HIGH_SPEED_LOW`, `QUALITY_HIGH_SPEED_HIGH`, `QUALITY_HIGH_SPEED_480P`, `QUALITY_HIGH_SPEED_720P`, `QUALITY_HIGH_SPEED_1080P`, `QUALITY_HIGH_SPEED_2160P`, `QUALITY_HIGH_SPEED_CIF`, `QUALITY_HIGH_SPEED_VGA`, or `QUALITY_HIGH_SPEED_4KDCI`

Returns
`EncoderProfiles` | null if there are no encoder profiles defined for the quality level for the given camera.

Throws
`IllegalArgumentException` | if quality is not one of the defined QUALITY_ values.

See also:

- `QUALITY_LOW`
- `QUALITY_HIGH`
- `QUALITY_QCIF`
- `QUALITY_CIF`
- `QUALITY_480P`
- `QUALITY_720P`
- `QUALITY_1080P`
- `QUALITY_2160P`
- `QUALITY_TIME_LAPSE_LOW`
- `QUALITY_TIME_LAPSE_HIGH`
- `QUALITY_TIME_LAPSE_QCIF`
- `QUALITY_TIME_LAPSE_CIF`
- `QUALITY_TIME_LAPSE_480P`
- `QUALITY_TIME_LAPSE_720P`
- `QUALITY_TIME_LAPSE_1080P`
- `QUALITY_TIME_LAPSE_2160P`
- `QUALITY_HIGH_SPEED_LOW`
- `QUALITY_HIGH_SPEED_HIGH`
- `QUALITY_HIGH_SPEED_480P`
- `QUALITY_HIGH_SPEED_720P`
- `QUALITY_HIGH_SPEED_1080P`
- `QUALITY_HIGH_SPEED_2160P`

### hasProfile

    public static boolean hasProfile (int cameraId,
                    int quality)

Returns true if a camcorder profile exists for the given camera at the given quality level.

When using the Camera 2 API in LEGACY mode (i.e. when `CameraCharacteristics.INFO_SUPPORTED_HARDWARE_LEVEL` is set to `CameraMetadata.INFO_SUPPORTED_HARDWARE_LEVEL_LEGACY`), `hasProfile(int)` may return `true` for unsupported resolutions. To ensure a a given resolution is supported in LEGACY mode, the configuration given in `CameraCharacteristics.SCALER_STREAM_CONFIGURATION_MAP` must contain the the resolution in the supported output sizes. The recommended way to check this is with `StreamConfigurationMap.getOutputSizes(Class)` with the class of the desired recording endpoint, and check that the desired resolution is contained in the list returned.

Parameters
`cameraId` | `int`: the id for the camera. Integer camera ids parsed from the list received by invoking `CameraManager#getCameraIdList` can be used as long as they are `CameraMetadata#REQUEST_AVAILABLE_CAPABILITIES_BACKWARD_COMPATIBLE` and not `EXTERNAL`.
`quality` | `int`: the target quality level for the camcorder profile

Returns
`boolean` |

See also:

- `CameraManager`
- `CameraCharacteristics`

### hasProfile

    public static boolean hasProfile (int quality)

Returns true if a camcorder profile exists for the first back-facing camera at the given quality level.

When using the Camera 2 API in `LEGACY` mode (i.e. when `CameraCharacteristics.INFO_SUPPORTED_HARDWARE_LEVEL` is set to `CameraMetadata.INFO_SUPPORTED_HARDWARE_LEVEL_LEGACY`), `hasProfile(int)` may return `true` for unsupported resolutions. To ensure a a given resolution is supported in LEGACY mode, the configuration given in `CameraCharacteristics.SCALER_STREAM_CONFIGURATION_MAP` must contain the the resolution in the supported output sizes. The recommended way to check this is with `StreamConfigurationMap.getOutputSizes(Class)` with the class of the desired recording endpoint, and check that the desired resolution is contained in the list returned.

Parameters
`quality` | `int`: the target quality level for the camcorder profile

Returns
`boolean` |

See also:

- `CameraManager`
- `CameraCharacteristics`

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*