# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Inherited Constants | Methods | Inherited Methods

# BluetoothGattServer

`public final class BluetoothGattServer`
`extends Object` `implements BluetoothProfile`

java.lang.Object
↳ | android.bluetooth.BluetoothGattServer

Public API for the Bluetooth GATT Profile server role.

This class provides Bluetooth GATT server role functionality, allowing applications to create Bluetooth Smart services and characteristics.

BluetoothGattServer is a proxy object for controlling the Bluetooth Service via IPC. Use `BluetoothManager#openGattServer` to get an instance of this class.

## Summary

### Inherited constants
From interface `android.bluetooth.BluetoothProfile`
`int` | `A2DP` A2DP profile.
`String` | `EXTRA_PREVIOUS_STATE` Extra for the connection state intents of the individual profiles.
`String` | `EXTRA_STATE` Extra for the connection state intents of the individual profiles.
`int` | `GATT` GATT
`int` | `GATT_SERVER` GATT_SERVER
`int` | `HEADSET` Headset and Handsfree profile
`int` | `HEALTH` This constant is deprecated. Health Device Profile (HDP) and MCAP protocol are no longer used. New apps should use Bluetooth Low Energy based solutions such as `BluetoothGatt`, `BluetoothAdapter#listenUsingL2capChannel()`, or `BluetoothDevice#createL2capChannel(int)`
`int` | `HEARING_AID` Hearing Aid Device
`int` | `HID_DEVICE` HID Device
`int` | `SAP`
`int` | `STATE_CONNECTED` The profile is in connected state
`int` | `STATE_CONNECTING` The profile is in connecting state
`int` | `STATE_DISCONNECTED` The profile is in disconnected state
`int` | `STATE_DISCONNECTING` The profile is in disconnecting state

### Public methods
`boolean` | `addService(BluetoothGattService service)` Add a service to the list of services to be hosted.
`void` | `cancelConnection(BluetoothDevice device)` Disconnects an established connection, or cancels a connection attempt currently in progress.
`void` | `clearServices()` Remove all services from the list of provided services.
`void` | `close()` Close this GATT server instance.
`boolean` | `connect(BluetoothDevice device, boolean autoConnect)` Initiate a connection to a Bluetooth GATT capable device.
`List<BluetoothDevice>` | `getConnectedDevices()` Not supported - please use `BluetoothManager#getConnectedDevices(int)` with `BluetoothProfile#GATT` as argument
`int` | `getConnectionState(BluetoothDevice device)` Not supported - please use `BluetoothManager#getConnectedDevices(int)` with `BluetoothProfile#GATT` as argument
`List<BluetoothDevice>` | `getDevicesMatchingConnectionStates(int[] states)` Not supported - please use `BluetoothManager#getDevicesMatchingConnectionStates(int, int[])` with `BluetoothProfile#GATT` as first argument
`BluetoothGattService` | `getService(UUID uuid)` Returns a `BluetoothGattService` from the list of services offered by this device.
`List<BluetoothGattService>` | `getServices()` Returns a list of GATT services offered by this device.
`boolean` | `notifyCharacteristicChanged(BluetoothDevice device, BluetoothGattCharacteristic characteristic, boolean confirm)` Send a notification or indication that a local characteristic has been updated.
`void` | `readPhy(BluetoothDevice device)` Read the current transmitter PHY and receiver PHY of the connection.
`boolean` | `removeService(BluetoothGattService service)` Removes a service from the list of services to be provided.
`boolean` | `sendResponse(BluetoothDevice device, int requestId, int status, int offset, byte[] value)` Send a response to a read or write request to a remote device.
`void` | `setPreferredPhy(BluetoothDevice device, int txPhy, int rxPhy, int phyOptions)` Set the preferred connection PHY for this app.

### Inherited methods
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.
From interface `android.bluetooth.BluetoothProfile`
`abstract List<BluetoothDevice>` | `getConnectedDevices()` Get connected devices for this specific profile.
`abstract int` | `getConnectionState(BluetoothDevice device)` Get the current connection state of the profile Requires `Manifest.permission.BLUETOOTH`
`abstract List<BluetoothDevice>` | `getDevicesMatchingConnectionStates(int[] states)` Get a list of devices that match any of the given connection states.

## Public methods

### addService

    public boolean addService (BluetoothGattService service)

Add a service to the list of services to be hosted.

Once a service has been addded to the list, the service and its included characteristics will be provided by the local device.

If the local device has already exposed services when this function is called, a service update notification will be sent to all clients.

The `BluetoothGattServerCallback#onServiceAdded` callback will indicate whether this service has been added successfully. Do not add another service before this callback.

Requires `Manifest.permission.BLUETOOTH` permission.

Parameters
`service` | `BluetoothGattService`: Service to be added to the list of services provided by this device.

Returns
`boolean` | true, if the request to add service has been initiated

### cancelConnection

    public void cancelConnection (BluetoothDevice device)

Disconnects an established connection, or cancels a connection attempt currently in progress.

Requires `Manifest.permission.BLUETOOTH` permission.

Parameters
`device` | `BluetoothDevice`: Remote device

### clearServices

    public void clearServices ()

Remove all services from the list of provided services.

Requires `Manifest.permission.BLUETOOTH` permission.

### close

    public void close ()

Close this GATT server instance. Application should call this method as early as possible after it is done with this GATT server.

### connect

    public boolean connect (BluetoothDevice device,
                    boolean autoConnect)

Initiate a connection to a Bluetooth GATT capable device.

The connection may not be established right away, but will be completed when the remote device is available. A `BluetoothGattServerCallback#onConnectionStateChange` callback will be invoked when the connection state changes as a result of this function.

The autoConnect parameter determines whether to actively connect to the remote device, or rather passively scan and finalize the connection when the remote device is in range/available. Generally, the first ever connection to a device should be direct (autoConnect set to false) and subsequent connections to known devices should be invoked with the autoConnect parameter set to true.

Requires `Manifest.permission.BLUETOOTH` permission.

Parameters
`device` | `BluetoothDevice`
`autoConnect` | `boolean`: Whether to directly connect to the remote device (false) or to automatically connect as soon as the remote device becomes available (true).

Returns
`boolean` | true, if the connection attempt was initiated successfully

### getConnectedDevices

    public List<BluetoothDevice> getConnectedDevices ()

Not supported - please use `BluetoothManager#getConnectedDevices(int)` with `BluetoothProfile#GATT` as argument

Returns
`List<BluetoothDevice>` | List of devices. The list will be empty on error.

Throws
`` | java.lang.UnsupportedOperationException

### getConnectionState

    public int getConnectionState (BluetoothDevice device)

Not supported - please use `BluetoothManager#getConnectedDevices(int)` with `BluetoothProfile#GATT` as argument

Parameters
`device` | `BluetoothDevice`: Remote bluetooth device.

Returns
`int` | State of the profile connection. One of `STATE_CONNECTED`, `STATE_CONNECTING`, `STATE_DISCONNECTED`, `STATE_DISCONNECTING` Value is `STATE_DISCONNECTED`, `STATE_CONNECTING`, `STATE_CONNECTED`, or `STATE_DISCONNECTING`

Throws
`` | java.lang.UnsupportedOperationException

### getDevicesMatchingConnectionStates

    public List<BluetoothDevice> getDevicesMatchingConnectionStates (int[] states)

Not supported - please use `BluetoothManager#getDevicesMatchingConnectionStates(int, int[])` with `BluetoothProfile#GATT` as first argument

Parameters
`states` | `int`: Array of states. States can be one of `BluetoothProfile.STATE_CONNECTED`, `BluetoothProfile.STATE_CONNECTING`, `BluetoothProfile.STATE_DISCONNECTED`, `BluetoothProfile.STATE_DISCONNECTING`,

Returns
`List<BluetoothDevice>` | List of devices. The list will be empty on error.

Throws
`` | java.lang.UnsupportedOperationException

### getService

    public BluetoothGattService getService (UUID uuid)

Returns a `BluetoothGattService` from the list of services offered by this device.

If multiple instances of the same service (as identified by UUID) exist, the first instance of the service is returned.

Requires `Manifest.permission.BLUETOOTH` permission.

Parameters
`uuid` | `UUID`: UUID of the requested service

Returns
`BluetoothGattService` | BluetoothGattService if supported, or null if the requested service is not offered by this device.

### getServices

    public List<BluetoothGattService> getServices ()

Returns a list of GATT services offered by this device.

An application must call `addService(BluetoothGattService)` to add a serice to the list of services offered by this device.

Requires `Manifest.permission.BLUETOOTH` permission.

Returns
`List<BluetoothGattService>` | List of services. Returns an empty list if no services have been added yet.

### notifyCharacteristicChanged

    public boolean notifyCharacteristicChanged (BluetoothDevice device,
                    BluetoothGattCharacteristic characteristic,
                    boolean confirm)

Send a notification or indication that a local characteristic has been updated.

A notification or indication is sent to the remote device to signal that the characteristic has been updated. This function should be invoked for every client that requests notifications/indications by writing to the "Client Configuration" descriptor for the given characteristic.

Requires `Manifest.permission.BLUETOOTH` permission.

Parameters
`device` | `BluetoothDevice`: The remote device to receive the notification/indication
`characteristic` | `BluetoothGattCharacteristic`: The local characteristic that has been updated
`confirm` | `boolean`: true to request confirmation from the client (indication), false to send a notification

Returns
`boolean` | true, if the notification has been triggered successfully

Throws
`` | java.lang.IllegalArgumentException

### readPhy

    public void readPhy (BluetoothDevice device)

Read the current transmitter PHY and receiver PHY of the connection. The values are returned in `BluetoothGattServerCallback#onPhyRead`

Parameters
`device` | `BluetoothDevice`: The remote device to send this response to

### removeService

    public boolean removeService (BluetoothGattService service)

Removes a service from the list of services to be provided.

Requires `Manifest.permission.BLUETOOTH` permission.

Parameters
`service` | `BluetoothGattService`: Service to be removed.

Returns
`boolean` | true, if the service has been removed

### sendResponse

    public boolean sendResponse (BluetoothDevice device,
                    int requestId,
                    int status,
                    int offset,
                    byte[] value)

Send a response to a read or write request to a remote device.

This function must be invoked in when a remote read/write request is received by one of these callback methods:

- `BluetoothGattServerCallback#onCharacteristicReadRequest`
- `BluetoothGattServerCallback#onCharacteristicWriteRequest`
- `BluetoothGattServerCallback#onDescriptorReadRequest`
- `BluetoothGattServerCallback#onDescriptorWriteRequest`

Requires `Manifest.permission.BLUETOOTH` permission.

Parameters
`device` | `BluetoothDevice`: The remote device to send this response to
`requestId` | `int`: The ID of the request that was received with the callback
`status` | `int`: The status of the request to be sent to the remote devices
`offset` | `int`: Value offset for partial read/write response
`value` | `byte`: The value of the attribute that was read/written (optional)

Returns
`boolean` |

### setPreferredPhy

    public void setPreferredPhy (BluetoothDevice device,
                    int txPhy,
                    int rxPhy,
                    int phyOptions)

Set the preferred connection PHY for this app. Please note that this is just a recommendation, whether the PHY change will happen depends on other applications peferences, local and remote controller capabilities. Controller can override these settings.

`BluetoothGattServerCallback#onPhyUpdate` will be triggered as a result of this call, even if no PHY change happens. It is also triggered when remote device updates the PHY.

Parameters
`device` | `BluetoothDevice`: The remote device to send this response to
`txPhy` | `int`: preferred transmitter PHY. Bitwise OR of any of `BluetoothDevice#PHY_LE_1M_MASK`, `BluetoothDevice#PHY_LE_2M_MASK`, and `BluetoothDevice#PHY_LE_CODED_MASK`.
`rxPhy` | `int`: preferred receiver PHY. Bitwise OR of any of `BluetoothDevice#PHY_LE_1M_MASK`, `BluetoothDevice#PHY_LE_2M_MASK`, and `BluetoothDevice#PHY_LE_CODED_MASK`.
`phyOptions` | `int`: preferred coding to use when transmitting on the LE Coded PHY. Can be one of `BluetoothDevice#PHY_OPTION_NO_PREFERRED`, `BluetoothDevice#PHY_OPTION_S2` or `BluetoothDevice#PHY_OPTION_S8`

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*