# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Constants | Inherited Methods

# AccessNetworkConstants.UtranBand

`public static final class AccessNetworkConstants.UtranBand`
`extends Object` ``

java.lang.Object
↳ | android.telephony.AccessNetworkConstants.UtranBand

Frequency bands for UTRAN. http://www.etsi.org/deliver/etsi_ts/125100_125199/125104/13.03.00_60/ts_125104v130p.pdf

## Summary

### Constants
`int` | `BAND_1`
`int` | `BAND_10`
`int` | `BAND_11`
`int` | `BAND_12`
`int` | `BAND_13`
`int` | `BAND_14`
`int` | `BAND_19`
`int` | `BAND_2`
`int` | `BAND_20`
`int` | `BAND_21`
`int` | `BAND_22`
`int` | `BAND_25`
`int` | `BAND_26`
`int` | `BAND_3`
`int` | `BAND_4`
`int` | `BAND_5`
`int` | `BAND_6`
`int` | `BAND_7`
`int` | `BAND_8`
`int` | `BAND_9`
`int` | `BAND_A` Band A 1900 - 1920 MHz: Uplink and downlink transmission 2010 - 2025 MHz: Uplink and downlink transmission
`int` | `BAND_B` Band B 1850 - 1910 MHz: Uplink and downlink transmission 1930 - 1990 MHz: Uplink and downlink transmission
`int` | `BAND_C` Band C 1910 - 1930 MHz: Uplink and downlink transmission
`int` | `BAND_D` Band D 2570 - 2620 MHz: Uplink and downlink transmission
`int` | `BAND_E` Band E 2300—2400 MHz: Uplink and downlink transmission
`int` | `BAND_F` Band F 1880 - 1920 MHz: Uplink and downlink transmission

### Inherited methods
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.

## Constants

### BAND_1

    public static final int BAND_1

Constant Value: 1 (0x00000001)

### BAND_10

    public static final int BAND_10

Constant Value: 10 (0x0000000a)

### BAND_11

    public static final int BAND_11

Constant Value: 11 (0x0000000b)

### BAND_12

    public static final int BAND_12

Constant Value: 12 (0x0000000c)

### BAND_13

    public static final int BAND_13

Constant Value: 13 (0x0000000d)

### BAND_14

    public static final int BAND_14

Constant Value: 14 (0x0000000e)

### BAND_19

    public static final int BAND_19

Constant Value: 19 (0x00000013)

### BAND_2

    public static final int BAND_2

Constant Value: 2 (0x00000002)

### BAND_20

    public static final int BAND_20

Constant Value: 20 (0x00000014)

### BAND_21

    public static final int BAND_21

Constant Value: 21 (0x00000015)

### BAND_22

    public static final int BAND_22

Constant Value: 22 (0x00000016)

### BAND_25

    public static final int BAND_25

Constant Value: 25 (0x00000019)

### BAND_26

    public static final int BAND_26

Constant Value: 26 (0x0000001a)

### BAND_3

    public static final int BAND_3

Constant Value: 3 (0x00000003)

### BAND_4

    public static final int BAND_4

Constant Value: 4 (0x00000004)

### BAND_5

    public static final int BAND_5

Constant Value: 5 (0x00000005)

### BAND_6

    public static final int BAND_6

Constant Value: 6 (0x00000006)

### BAND_7

    public static final int BAND_7

Constant Value: 7 (0x00000007)

### BAND_8

    public static final int BAND_8

Constant Value: 8 (0x00000008)

### BAND_9

    public static final int BAND_9

Constant Value: 9 (0x00000009)

### BAND_A

    public static final int BAND_A

Band A 1900 - 1920 MHz: Uplink and downlink transmission 2010 - 2025 MHz: Uplink and downlink transmission

Constant Value: 101 (0x00000065)

### BAND_B

    public static final int BAND_B

Band B 1850 - 1910 MHz: Uplink and downlink transmission 1930 - 1990 MHz: Uplink and downlink transmission

Constant Value: 102 (0x00000066)

### BAND_C

    public static final int BAND_C

Band C 1910 - 1930 MHz: Uplink and downlink transmission

Constant Value: 103 (0x00000067)

### BAND_D

    public static final int BAND_D

Band D 2570 - 2620 MHz: Uplink and downlink transmission

Constant Value: 104 (0x00000068)

### BAND_E

    public static final int BAND_E

Band E 2300—2400 MHz: Uplink and downlink transmission

Constant Value: 105 (0x00000069)

### BAND_F

    public static final int BAND_F

Band F 1880 - 1920 MHz: Uplink and downlink transmission

Constant Value: 106 (0x0000006a)

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*