# Print output for @column tags ?>
Developers

- Design
- Develop
- Distribute

Developer Console

## Most visited

## Recently visited

## Results for

Summary: Enums | Methods | Inherited Methods

# ColorSpace.Named

`public static final enum ColorSpace.Named`
`` `extends Enum<ColorSpace.Named>` ``

java.lang.Object
↳ | java.lang.Enum<android.graphics.ColorSpace.Named>
| ↳ | android.graphics.ColorSpace.Named

List of common, named color spaces. A corresponding instance of `ColorSpace` can be obtained by calling `ColorSpace#get(Named)`:

     ColorSpace cs = ColorSpace.get(ColorSpace.Named.DCI_P3);

The properties of each color space are described below (see `sRGB` for instance). When applicable, the color gamut of each color space is compared to the color gamut of sRGB using a CIE 1931 xy chromaticity diagram. This diagram shows the location of the color space's primaries and white point.

See also:

- `ColorSpace.get(Named)`

## Summary

### Enum values
`ColorSpace.Named` | `ACES` `ColorSpace.Rgb` color space ACES standardized as SMPTE ST 2065-1:2012.
`ColorSpace.Named` | `ACESCG` `ColorSpace.Rgb` color space ACEScg standardized as Academy S-2014-004.
`ColorSpace.Named` | `ADOBE_RGB` `ColorSpace.Rgb` color space Adobe RGB (1998).
`ColorSpace.Named` | `BT2020` `ColorSpace.Rgb` color space BT.2020 standardized as Rec.
`ColorSpace.Named` | `BT709` `ColorSpace.Rgb` color space BT.709 standardized as Rec.
`ColorSpace.Named` | `CIE_LAB` `Model#LAB` color space CIE L*a*b*.
`ColorSpace.Named` | `CIE_XYZ` `Model#XYZ` color space CIE XYZ.
`ColorSpace.Named` | `DCI_P3` `ColorSpace.Rgb` color space DCI-P3 standardized as SMPTE RP 431-2-2007.
`ColorSpace.Named` | `DISPLAY_P3` `ColorSpace.Rgb` color space Display P3 based on SMPTE RP 431-2-2007 and IEC 61966-2.1:1999.
`ColorSpace.Named` | `EXTENDED_SRGB` `ColorSpace.Rgb` color space scRGB-nl standardized as IEC 61966-2-2:2003.
`ColorSpace.Named` | `LINEAR_EXTENDED_SRGB` `ColorSpace.Rgb` color space scRGB standardized as IEC 61966-2-2:2003.
`ColorSpace.Named` | `LINEAR_SRGB` `ColorSpace.Rgb` color space sRGB standardized as IEC 61966-2.1:1999.
`ColorSpace.Named` | `NTSC_1953` `ColorSpace.Rgb` color space NTSC, 1953 standard.
`ColorSpace.Named` | `PRO_PHOTO_RGB` `ColorSpace.Rgb` color space ProPhoto RGB standardized as ROMM RGB ISO 22028-2:2013.
`ColorSpace.Named` | `SMPTE_C` `ColorSpace.Rgb` color space SMPTE C.
`ColorSpace.Named` | `SRGB` `ColorSpace.Rgb` color space sRGB standardized as IEC 61966-2.1:1999.

### Public methods
`static ColorSpace.Named` | `valueOf(String name)`
`static final Named[]` | `values()`

### Inherited methods
From class `java.lang.Enum`
`final Object` | `clone()` Throws CloneNotSupportedException.
`final int` | `compareTo(ColorSpace.Named o)` Compares this enum with the specified object for order.
`final boolean` | `equals(Object other)` Returns true if the specified object is equal to this enum constant.
`final void` | `finalize()` enum classes cannot have finalize methods.
`final Class<ColorSpace.Named>` | `getDeclaringClass()` Returns the Class object corresponding to this enum constant's enum type.
`final int` | `hashCode()` Returns a hash code for this enum constant.
`final String` | `name()` Returns the name of this enum constant, exactly as declared in its enum declaration.
`final int` | `ordinal()` Returns the ordinal of this enumeration constant (its position in its enum declaration, where the initial constant is assigned an ordinal of zero).
`String` | `toString()` Returns the name of this enum constant, as contained in the declaration.
`static <T extends Enum<T>> T` | `valueOf(Class<T> enumType, String name)` Returns the enum constant of the specified enum type with the specified name.
From class `java.lang.Object`
`Object` | `clone()` Creates and returns a copy of this object.
`boolean` | `equals(Object obj)` Indicates whether some other object is "equal to" this one.
`void` | `finalize()` Called by the garbage collector on an object when garbage collection determines that there are no more references to the object.
`final Class<?>` | `getClass()` Returns the runtime class of this `Object`.
`int` | `hashCode()` Returns a hash code value for the object.
`final void` | `notify()` Wakes up a single thread that is waiting on this object's monitor.
`final void` | `notifyAll()` Wakes up all threads that are waiting on this object's monitor.
`String` | `toString()` Returns a string representation of the object.
`final void` | `wait(long timeout, int nanos)` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object, or some other thread interrupts the current thread, or a certain amount of real time has elapsed.
`final void` | `wait(long timeout)` Causes the current thread to wait until either another thread invokes the `notify()` method or the `notifyAll()` method for this object, or a specified amount of time has elapsed.
`final void` | `wait()` Causes the current thread to wait until another thread invokes the `notify()` method or the `notifyAll()` method for this object.
From interface `java.lang.Comparable`
`abstract int` | `compareTo(ColorSpace.Named o)` Compares this object with the specified object for order.

## Enum values

### ACES

    public static final ColorSpace.Named ACES

`ColorSpace.Rgb` color space ACES standardized as SMPTE ST 2065-1:2012.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.73470 | 0.00000 | 0.00010 | 0.32168
y | 0.26530 | 1.00000 | -0.07700 | 0.33767
Property | Value
Name | SMPTE ST 2065-1:2012 ACES
CIE standard illuminant | D60
Opto-electronic transfer function (OETF) | \(C_{ACES} = C_{linear}\)
Electro-optical transfer function (EOTF) | \(C_{linear} = C_{ACES}\)
Range | \([-65504.0, 65504.0]\)

ACES (orange) vs sRGB (white)

### ACESCG

    public static final ColorSpace.Named ACESCG

`ColorSpace.Rgb` color space ACEScg standardized as Academy S-2014-004.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.713 | 0.165 | 0.128 | 0.32168
y | 0.293 | 0.830 | 0.044 | 0.33767
Property | Value
Name | Academy S-2014-004 ACEScg
CIE standard illuminant | D60
Opto-electronic transfer function (OETF) | \(C_{ACEScg} = C_{linear}\)
Electro-optical transfer function (EOTF) | \(C_{linear} = C_{ACEScg}\)
Range | \([-65504.0, 65504.0]\)

ACEScg (orange) vs sRGB (white)

### ADOBE_RGB

    public static final ColorSpace.Named ADOBE_RGB

`ColorSpace.Rgb` color space Adobe RGB (1998).

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.64 | 0.21 | 0.15 | 0.3127
y | 0.33 | 0.71 | 0.06 | 0.3290
Property | Value
Name | Adobe RGB (1998)
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(C_{RGB} = C_{linear}^{\frac{1}{2.2}}\)
Electro-optical transfer function (EOTF) | \(C_{linear} = C_{RGB}^{2.2}\)
Range | \([0..1]\)

Adobe RGB (orange) vs sRGB (white)

### BT2020

    public static final ColorSpace.Named BT2020

`ColorSpace.Rgb` color space BT.2020 standardized as Rec. ITU-R BT.2020-1.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.708 | 0.170 | 0.131 | 0.3127
y | 0.292 | 0.797 | 0.046 | 0.3290
Property | Value
Name | Rec. ITU-R BT.2020-1
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(\begin{equation} C_{BT2020} = \begin{cases} 4.5 \times C_{linear} & C_{linear} \lt 0.0181 \\\ 1.0993 \times C_{linear}^{\frac{1}{2.2}} - 0.0993 & C_{linear} \ge 0.0181 \end{cases} \end{equation}\)
Electro-optical transfer function (EOTF) | \(\begin{equation} C_{linear} = \begin{cases}\frac{C_{BT2020}}{4.5} & C_{BT2020} \lt 0.08145 \\\ \left( \frac{C_{BT2020} + 0.0993}{1.0993} \right) ^{2.2} & C_{BT2020} \ge 0.08145 \end{cases} \end{equation}\)
Range | \([0..1]\)

BT.2020 (orange) vs sRGB (white)

### BT709

    public static final ColorSpace.Named BT709

`ColorSpace.Rgb` color space BT.709 standardized as Rec. ITU-R BT.709-5.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.640 | 0.300 | 0.150 | 0.3127
y | 0.330 | 0.600 | 0.060 | 0.3290
Property | Value
Name | Rec. ITU-R BT.709-5
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(\begin{equation} C_{BT709} = \begin{cases} 4.5 \times C_{linear} & C_{linear} \lt 0.018 \\\ 1.099 \times C_{linear}^{\frac{1}{2.2}} - 0.099 & C_{linear} \ge 0.018 \end{cases} \end{equation}\)
Electro-optical transfer function (EOTF) | \(\begin{equation} C_{linear} = \begin{cases}\frac{C_{BT709}}{4.5} & C_{BT709} \lt 0.081 \\\ \left( \frac{C_{BT709} + 0.099}{1.099} \right) ^{2.2} & C_{BT709} \ge 0.081 \end{cases} \end{equation}\)
Range | \([0..1]\)

BT.709

### CIE_LAB

    public static final ColorSpace.Named CIE_LAB

`Model#LAB` color space CIE L*a*b*. This color space uses CIE XYZ D50 as a profile conversion space.

Property | Value
--- | ---
Name | Generic L*a*b*
CIE standard illuminant | D50
Range | \(L: [0.0, 100.0], a: [-128, 128], b: [-128, 128]\)

### CIE_XYZ

    public static final ColorSpace.Named CIE_XYZ

`Model#XYZ` color space CIE XYZ. This color space assumes standard illuminant D50 as its white point.

Property | Value
--- | ---
Name | Generic XYZ
CIE standard illuminant | D50
Range | \([-2.0, 2.0]\)

### DCI_P3

    public static final ColorSpace.Named DCI_P3

`ColorSpace.Rgb` color space DCI-P3 standardized as SMPTE RP 431-2-2007.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.680 | 0.265 | 0.150 | 0.314
y | 0.320 | 0.690 | 0.060 | 0.351
Property | Value
Name | SMPTE RP 431-2-2007 DCI (P3)
CIE standard illuminant | N/A
Opto-electronic transfer function (OETF) | \(C_{P3} = C_{linear}^{\frac{1}{2.6}}\)
Electro-optical transfer function (EOTF) | \(C_{linear} = C_{P3}^{2.6}\)
Range | \([0..1]\)

DCI-P3 (orange) vs sRGB (white)

### DISPLAY_P3

    public static final ColorSpace.Named DISPLAY_P3

`ColorSpace.Rgb` color space Display P3 based on SMPTE RP 431-2-2007 and IEC 61966-2.1:1999.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.680 | 0.265 | 0.150 | 0.3127
y | 0.320 | 0.690 | 0.060 | 0.3290
Property | Value
Name | Display P3
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(\begin{equation} C_{DisplayP3} = \begin{cases} 12.92 \times C_{linear} & C_{linear} \lt 0.0030186 \\\ 1.055 \times C_{linear}^{\frac{1}{2.4}} - 0.055 & C_{linear} \ge 0.0030186 \end{cases} \end{equation}\)
Electro-optical transfer function (EOTF) | \(\begin{equation} C_{linear} = \begin{cases}\frac{C_{DisplayP3}}{12.92} & C_{sRGB} \lt 0.04045 \\\ \left( \frac{C_{DisplayP3} + 0.055}{1.055} \right) ^{2.4} & C_{sRGB} \ge 0.04045 \end{cases} \end{equation}\)
Range | \([0..1]\)

Display P3 (orange) vs sRGB (white)

### EXTENDED_SRGB

    public static final ColorSpace.Named EXTENDED_SRGB

`ColorSpace.Rgb` color space scRGB-nl standardized as IEC 61966-2-2:2003.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.640 | 0.300 | 0.150 | 0.3127
y | 0.330 | 0.600 | 0.060 | 0.3290
Property | Value
Name | scRGB-nl IEC 61966-2-2:2003
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(\begin{equation} C_{scRGB} = \begin{cases} sign(C_{linear}) 12.92 \times \left| C_{linear} \right| & \left| C_{linear} \right| \lt 0.0031308 \\\ sign(C_{linear}) 1.055 \times \left| C_{linear} \right| ^{\frac{1}{2.4}} - 0.055 & \left| C_{linear} \right| \ge 0.0031308 \end{cases} \end{equation}\)
Electro-optical transfer function (EOTF) | \(\begin{equation} C_{linear} = \begin{cases}sign(C_{scRGB}) \frac{\left| C_{scRGB} \right|}{12.92} & \left| C_{scRGB} \right| \lt 0.04045 \\\ sign(C_{scRGB}) \left( \frac{\left| C_{scRGB} \right| + 0.055}{1.055} \right) ^{2.4} & \left| C_{scRGB} \right| \ge 0.04045 \end{cases} \end{equation}\)
Range | \([-0.799..2.399[\)

Extended sRGB (orange) vs sRGB (white)

### LINEAR_EXTENDED_SRGB

    public static final ColorSpace.Named LINEAR_EXTENDED_SRGB

`ColorSpace.Rgb` color space scRGB standardized as IEC 61966-2-2:2003.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.640 | 0.300 | 0.150 | 0.3127
y | 0.330 | 0.600 | 0.060 | 0.3290
Property | Value
Name | scRGB IEC 61966-2-2:2003
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(C_{scRGB} = C_{linear}\)
Electro-optical transfer function (EOTF) | \(C_{linear} = C_{scRGB}\)
Range | \([-0.5..7.499[\)

Extended sRGB (orange) vs sRGB (white)

### LINEAR_SRGB

    public static final ColorSpace.Named LINEAR_SRGB

`ColorSpace.Rgb` color space sRGB standardized as IEC 61966-2.1:1999.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.640 | 0.300 | 0.150 | 0.3127
y | 0.330 | 0.600 | 0.060 | 0.3290
Property | Value
Name | sRGB IEC61966-2.1 (Linear)
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(C_{sRGB} = C_{linear}\)
Electro-optical transfer function (EOTF) | \(C_{linear} = C_{sRGB}\)
Range | \([0..1]\)

sRGB

### NTSC_1953

    public static final ColorSpace.Named NTSC_1953

`ColorSpace.Rgb` color space NTSC, 1953 standard.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.67 | 0.21 | 0.14 | 0.310
y | 0.33 | 0.71 | 0.08 | 0.316
Property | Value
Name | NTSC (1953)
CIE standard illuminant | C
Opto-electronic transfer function (OETF) | \(\begin{equation} C_{BT709} = \begin{cases} 4.5 \times C_{linear} & C_{linear} \lt 0.018 \\\ 1.099 \times C_{linear}^{\frac{1}{2.2}} - 0.099 & C_{linear} \ge 0.018 \end{cases} \end{equation}\)
Electro-optical transfer function (EOTF) | \(\begin{equation} C_{linear} = \begin{cases}\frac{C_{BT709}}{4.5} & C_{BT709} \lt 0.081 \\\ \left( \frac{C_{BT709} + 0.099}{1.099} \right) ^{2.2} & C_{BT709} \ge 0.081 \end{cases} \end{equation}\)
Range | \([0..1]\)

NTSC 1953 (orange) vs sRGB (white)

### PRO_PHOTO_RGB

    public static final ColorSpace.Named PRO_PHOTO_RGB

`ColorSpace.Rgb` color space ProPhoto RGB standardized as ROMM RGB ISO 22028-2:2013.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.7347 | 0.1596 | 0.0366 | 0.3457
y | 0.2653 | 0.8404 | 0.0001 | 0.3585
Property | Value
Name | ROMM RGB ISO 22028-2:2013
CIE standard illuminant | D50
Opto-electronic transfer function (OETF) | \(\begin{equation} C_{ROMM} = \begin{cases} 16 \times C_{linear} & C_{linear} \lt 0.001953 \\\ C_{linear}^{\frac{1}{1.8}} & C_{linear} \ge 0.001953 \end{cases} \end{equation}\)
Electro-optical transfer function (EOTF) | \(\begin{equation} C_{linear} = \begin{cases}\frac{C_{ROMM}}{16} & C_{ROMM} \lt 0.031248 \\\ C_{ROMM}^{1.8} & C_{ROMM} \ge 0.031248 \end{cases} \end{equation}\)
Range | \([0..1]\)

ProPhoto RGB (orange) vs sRGB (white)

### SMPTE_C

    public static final ColorSpace.Named SMPTE_C

`ColorSpace.Rgb` color space SMPTE C.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.630 | 0.310 | 0.155 | 0.3127
y | 0.340 | 0.595 | 0.070 | 0.3290
Property | Value
Name | SMPTE-C RGB
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(\begin{equation} C_{BT709} = \begin{cases} 4.5 \times C_{linear} & C_{linear} \lt 0.018 \\\ 1.099 \times C_{linear}^{\frac{1}{2.2}} - 0.099 & C_{linear} \ge 0.018 \end{cases} \end{equation}\)
Electro-optical transfer function (EOTF) | \(\begin{equation} C_{linear} = \begin{cases}\frac{C_{BT709}}{4.5} & C_{BT709} \lt 0.081 \\\ \left( \frac{C_{BT709} + 0.099}{1.099} \right) ^{2.2} & C_{BT709} \ge 0.081 \end{cases} \end{equation}\)
Range | \([0..1]\)

SMPTE-C (orange) vs sRGB (white)

### SRGB

    public static final ColorSpace.Named SRGB

`ColorSpace.Rgb` color space sRGB standardized as IEC 61966-2.1:1999.

Chromaticity | Red | Green | Blue | White point
--- | --- | --- | --- | ---
x | 0.640 | 0.300 | 0.150 | 0.3127
y | 0.330 | 0.600 | 0.060 | 0.3290
Property | Value
Name | sRGB IEC61966-2.1
CIE standard illuminant | D65
Opto-electronic transfer function (OETF) | \(\begin{equation} C_{sRGB} = \begin{cases} 12.92 \times C_{linear} & C_{linear} \lt 0.0031308 \\\ 1.055 \times C_{linear}^{\frac{1}{2.4}} - 0.055 & C_{linear} \ge 0.0031308 \end{cases} \end{equation}\)
Electro-optical transfer function (EOTF) | \(\begin{equation} C_{linear} = \begin{cases}\frac{C_{sRGB}}{12.92} & C_{sRGB} \lt 0.04045 \\\ \left( \frac{C_{sRGB} + 0.055}{1.055} \right) ^{2.4} & C_{sRGB} \ge 0.04045 \end{cases} \end{equation}\)
Range | \([0..1]\)

sRGB

## Public methods

### valueOf

    public static ColorSpace.Named valueOf (String name)

Parameters
`name` | `String`

Returns
`ColorSpace.Named` |

### values

    public static final Named[] values ()

Returns
`Named[]` |

Full name *
Email address *
Company / developer name
One of your Play Store app URLs *
Which best describes your business:*
Apps
Games
Apps & Games
*
*